**SUPPLY**

**+5V**

**KEY INPUT**

**BUZZER FOR WARNING**

**AND INDICATION**

**LED FOR WARNING**

**AND INDICATION**

**SW 1**

**SW 2**

**BUZZER**

**LED**

**DOOR STATUS ECU (HARDWARE I/P)**

**CAN\_INPUT**

PIC 18F458