**LED AND BUZZER ON AND OFF FOR 3 TIMES**

**3rd WRONG ATTEMPT**

**BUZZER ON CONTINUOSLY**

**2nd WRONG ATTEMPT**

**BUZZER ON AND OFF FOR 6 TIMES**

**1st WRONG ATTEMPT**

**BUZZER ON AND OFF FOR 3 TIMES**

**LED AND BUZZER ON AND OFF FOR 1 TIMES**

**INVALID ATTEMPT**

**UNLOCK**

**LOCK**

**READTING DATA FROM EEPROM**

**WRITING DATA INTO EEPROM**

**READ DATA STORED FROM CAN**

**WRITE DATA INTO CAN**

**MASK**

* **CANCON**
* **RX**
* **SIDL**
* **SIDH**

**FILTER**

* **CANCON**
* **RX**
* **SIDL**
* **SIDH**

**Set\_Baud rate()**

**CAWN**

**BRGWN**

**CIOCON**

**Delay**

**SYS\_init()**

**GIE**

**PEIE**

**Delay**

**CAN\_init()**

**TRIS**

**RX**

**RX**